|  |
| --- |
| **C:\Users\jeanne.waldowski\Dropbox\Rain Check\Logos & Graphics\Rain Check Logo-01.png permeable paver Consultation report** |

|  |  |  |  |
| --- | --- | --- | --- |
| **CLIENT information** | | | |
| Participant Name: |  | | |
| Street Address: |  | | |
| **cONTRACTOR information** | | | |
| Contractor Name |  | | |
| Consultation Date/Time |  | | |
| **Participant interview** | | **Yes** | **No** |
| Does your basement get wet? | |  |  |
| Do you have a sump pump in the basement? | |  |  |
| Are there any problems with roof drainage/leakage? | |  |  |
| Are there any problems with gutters/downspouts/risers? | |  |  |
| Do you experience ponding or stagnant water in your yard? | |  |  |
| Do you have any other drainage issues? | |  |  |
| If the participant answered “yes” to any of the above, please provide detail below: | | | |
| Ask participant for access to the basement. If access is denied, end consultation.  Please look for any obvious signs of moisture, and take photos as necessary (minimum of 2). Submit these to Zach Popkin along with this report. | | | |

These criteria must be met to install permeable paving:

Permeable paving will be installed in place of existing impervious surface.

Areas designated for permeable paving do **not** accept runoff from other areas (i.e. direct rainfall only is allowed).

If the basement is wet, the permeable pavement is at least 10 ft away from the basement wall.

The tool manages stormwater that would otherwise run into the sewer.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Feasibility** | | | **Yes** | | **No** |
| Is the installation of a permeable paver project feasible on the property? | | |  | |  |
| If not, please explain:  If not, are any other Rain Check tools feasible on this property? | | | | | |
| **INstallation Details** | | | | | |
| Dimensions of proposed paver project: | Width: | Length: | | Depth: | |
| Describe the installation site: | | | | | |
| Installing waterproof liner? (water proof liner is required when system abuts building wall) | | | | | |
| Estimated Storage Volume: (sq.ft. surface area) X 0.935 = gallons | | | | | |
| Estimated start date: | | | | | |

Please attach a detailed estimate, including

Price points: the total, Rain Check subsidy, and balance (homeowner portion)

Non-Rain Check work scope

Product detail (brand, color, shape)

Submit this form, site sketch, photo form, and estimate to Zach Popkin: [RainCheck@pennhort.org](mailto:zpopkin@pennhort.org)